C17 Circuits power profile Summary:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Circuit** | **Internal power (uW)** | **Switching power (uW)** | **Leakage power (pW)** | **Total power (uW)** |
| c17 | 0.9256 | 0.1137 | 7.72E+04 | 1.1165 |
| c17 Trojan 1 location 1 | 0 | 0.1119 | 0 | 0.1119 |
| c17 Trojan 1 location 2 | 0 | 0.1265 | 0 | 0.1265 |
| c17 Trojan 2 location 1 | 0 | 0.1017 | 0 | 0.1017 |
| c17 Trojan 2 location 2 | 0 | 0.1162 | 0 | 0.1162 |

C17 Circuits vs Total Power (uW):

C499 Circuits power profile Summary:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Circuit** | **Internal power (uW)** | **Switching power (uW)** | **Leakage power (pW)** | **Total power (uW)** |
| c499 | 0 | 8.7305 | 0 | 8.7305 |
| c499 trojan 1 location 1 | 0 | 8.4206 | 0 | 8.4206 |
| c499 trojan 1 location 2 | 0 | 8.5899 | 0 | 8.5899 |
| c499 trojan 2 location 1 | 0 | 8.5988 | 0 | 8.5988 |
| c499 trojan 2 location 2 | 0 | 8.6538 | 0 | 8.6538 |

C499 Circuits vs Total Power (uW)